Installing the Seeeduino XIAO configuration into Arduino IDE

Open the Prefrences tab in the Arduino IDE …. **File -> Prefrences**

Graphical user interface

Description automatically generated

Once open, proceed to the the “**Additional Boards Manager URLs:**” window.

Insert the following URL as a new line:

*https://files.seeedstudio.com/arduino/package\_seeeduino\_boards\_index.json*

Graphical user interface, text, application

Description automatically generated

Press “**OK**” and close the prefrences menu

Open the Tools tab in the Arduino IDE …. **Tools -> Board: -> Boards Manager…**

Graphical user interface, application

Description automatically generated

In the Boards Manager window, search for “seeed” in the upper field.

Find and Install the “Seeed SAMD Boards” package.

Graphical user interface, text, application, email

Description automatically generated

Once installed, you will find the “Seeeduino XIAO” board in the selection fields

Graphical user interface, application

Description automatically generated

For Additional Information, follow the page below:

<https://wiki.seeedstudio.com/Seeeduino-XIAO/#circuitpython-on-seeeduino-xiao>